**ATTACHMENT 1 – PASSENGER VEHICLES**

|  |
| --- |
| UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*  **MODEL YEAR 2021 OR NEWER: MID-SIZE; 4-DOOR SEDAN; REGULAR UNLEADED FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  110 inches to 113 inches |
| **OVERALL LENGTH:**  190 inches to 194.2 inches |
| **ENGINE:**  1.5 liter minimum |
| 4 cylinder minimum |
| Gasoline |
| **TRANSMISSION:**  Automatic |
| **DRIVETRAIN:**  Front Wheel Drive |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Four (4) |
| Manufacturer’s Standard Radial All Season |
| Tire Inflation and Sealant Kit OR Tire Tools and Compact Jack must be included |
| **SEATS:**  Cloth |
| Manufacturer’s Standard Front Seats |
| Manufacturer’s Standard Rear Bench Type Seat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Two (2) Sets of Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Malibu or other make/model equivalent** |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

AWD Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*  **MODEL YEAR 2021 OR NEWER: FULL-SIZE; 4-DOOR SEDAN; REGULAR UNLEADED FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  111 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **OVERALL LENGTH:**  198 inches minimum |
| **ENGINE:**  2.0 liter minimum |
| 4 cylinder minimum |
| Gasoline |
| **TRANSMISSION:**  Automatic |
| **DRIVETRAIN:**  Front Wheel Drive  (Rear wheel drive shall **NOT** be acceptable) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard Radial All Season |
| Compact Spare Acceptable for 5th tire |
| Tire Tools and Compact Jack Included |
| **SEATS:**  Cloth |
| Manufacturer’s Standard Front Seats |
| Manufacturer’s Standard Rear Bench Type Seat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |

|  |
| --- |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Two (2) Sets of Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Dodge Charger, Chrysler 300 or other make/model equivalent** |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

AWD Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*  **MODEL YEAR 2021 OR NEWER: COMPACT; 4-DOOR; ELECTRIC** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  102 inches to 105 inches |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **OVERALL LENGTH:**  Minimum of 163” |
| **DRIVETRAIN:**  Front Wheel Drive |
| **BATTERY:**  Lithium-Ion Battery Pack System |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Four (4) |
| Manufacturer’s Standard Radial All Season |
| Tire Inflation and Sealant Kit, Tire Tools and Compact Jack, OR ***Self Seal Tires*** must be included |
| **SEATS:**  Cloth |
| Manufacturer Standard Front Seats |
| Manufacturer Standard Rear Bench Type Seat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys with Key FOBS or Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |  |
| --- | --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: COMPACT; CROSSOVER; REGULAR UNLEADED FUEL** | |
| **Minimum Mandatory Specifications** | |
| **WHEELBASE:**  98.5 inches to 102 inches |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **OVERALL LENGTH:**  161 inches to 168 inches |
| **ENGINE:**  1.4 liter minimum |
| 4 cylinder minimum |
| Gasoline |
| **TRANSMISSION:**  Automatic |
| **DRIVETRAIN:**  All Wheel Drive or Four wheel drive |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Four (4) |
| Manufacturer’s Standard All Season |
| Tire Inflation and Sealant Kit OR Tire Tools and Compact Jack must be included |
| **SEATS:**  Cloth |
| Manufacturer’s Standard Front Seats |
| Manufacturer’s Standard Rear Bench Type Seat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Two (2) Sets of Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Trax, Ford Ecosport or other make/model equivalent** |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Front Wheel Drive

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |  |  |
| --- | --- | --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: SMALL SPORT UTILITY VEHICLE; 4X4; HYBRID** | | |
| **Minimum Mandatory Specifications** | | |
| **WHEELBASE:**  103.8 to 106.7 inches |
| **ENGINE:**  1.4 liter minimum |
| 4 cylinder maximum |
| **TRANSMISSION:**  4 speed minimum |
| Automatic |
| **DRIVETRAIN:**  Four (4) Wheel Drive/All Wheel Drive |
| **BATTERY:**  Lithium-Ion Battery Pack System |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating | |
| **RADIO:**  Manufacturer’s Standard | |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements | |
| Automatic Speed Control | |
| Daytime Running Lamps | |
| Tilt Wheel | |
| Electric Rear Window Defroster | |
| Power Windows (front and back) | |
| Power Door Locks | |
| Exterior Mirrors with interior remote adjustment | |
| Manufacturer’s Standard Cloth Front and Rear Seats | |
| Manufacturer Standard Floor Mats (front and rear) | |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters | |
| **If model proposed is flex fuel (E-85 capable):**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) | |
| **EXTERIOR COLORS:**  Manufacturer’s Standard | |
| **REFERENCE MODELS: Ford Escape Hybrid or other make/model equivalent** | | |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: SMALL SPORT UTILITY VEHICLE; 4X4** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  103.8 to 106.7 inches |
| **ENGINE:**  1.4 liter minimum |
| 3 cylinder minimum |
| **TRANSMISSION:**  4 speed minimum |
| Automatic |
| **DRIVETRAIN:**  Four (4) Wheel Drive (All Wheel Drive is NOT acceptable) |
| **TRANSFER CASE:**  Manufacturer’s Standard for Specific Transmission |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Cloth Front and Rear Seats |
| Manufacturer Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |

|  |  |
| --- | --- |
| **If model proposed is flex fuel (E-85 capable):**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |  |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Bronco Sport, Jeep Compass, Jeep Cherokee or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

FFV Fuel (E-85) Capable Model

Off-Road Package

Front Wheel Drive (FWD) Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |  |  |
| --- | --- | --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: MID-SIZE/STANDARD SPORT UTILITY VEHICLE;**  **4X4, REGULAR FUEL** | | |
| **Minimum Mandatory Specifications** | | |
| **WHEELBASE:**  114 inches minimum |
| **ENGINE:**  2.3 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**  4-Speed minimum |
| Automatic |
| **DRIVETRAIN:**  Four (4) Wheel Drive (All Wheel Drive is NOT acceptable) |
| **TRANSFER CASE:**  Manufacturer’s Standard for Specific Transmission |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |  | |
| **STEERING:**  Power Steering |  | |
| **TIRES:**  Five (5) |  | |
| Manufacturer’s Standard All Season |  | |
| Compact Spare Acceptable for 5th tire |  | |
| Tire tools and jack required |  | |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating | | |
| **RADIO:**  Manufacturer’s Standard | | |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements | | |
| Automatic Speed Control | | |
| Daytime Running Lamps | | |
| Tilt Wheel | | |
| Electric Rear Window Defroster | | |
| Power Windows (front and back) | | |
| Power Door Locks | | |
| Exterior Mirrors with interior remote adjustment | | |
| Manufacturer’s Standard Cloth Front and Rear Seats | | |
| Manufacturer’s Standard Floor Mats (front and rear) | | |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless  Entry Transmitters | | |
| **If model proposed is flex fuel (E-85 capable):**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) | | |
| **EXTERIOR COLORS:**  Manufacturer’s Standard | |
| **REFERENCE MODELS: Ford Explorer, Jeep Grand Cherokee, or other make/model equivalent** | | |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

Off-Road Package

Special Service (Police, etc.) Package Upgrade

Two (2) Wheel Drive Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: MID-SIZE/STANDARD SPORT UTILITY VEHICLE;**  **4X4, ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  114 inches minimum |
| **ENGINE:**  3.0 liter minimum, **Flex Fuel Capable** |
| 6 cylinder minimum |
| **TRANSMISSION:**  4-Speed minimum |
| Automatic |
| **DRIVETRAIN:**  Four (4) Wheel Drive (All Wheel Drive is NOT acceptable) |
| **TRANSFER CASE:**  Manufacturer’s Standard for Specific Transmission |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Cloth Front and Rear Seats |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Explorer or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

Off-Road Package

Special Service (Police, etc.) Package Upgrade

Two (2) Wheel Drive Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |  |
| --- | --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: MID-SIZE/STANDARD SPORT UTILITY VEHICLE; 4X4; HYBRID** | |
| **Minimum Mandatory Specifications** | |
| **WHEELBASE:**  119 inches minimum |
| **ENGINE:**  2.3 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**  4-Speed minimum |
| Automatic |
| **BATTERY:**  Lithium-Ion Battery Pack System |
| **DRIVETRAIN:**  Four (4) Wheel Drive (All Wheel Drive is NOT acceptable) |
| **TRANSFER CASE:**  Manufacturer’s Standard for Specific Transmission |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Backup Camera |
| Daytime Running Lamps |
| Automatic Speed Control |
| Backup Camera |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Cloth Front and Rear Seats |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless  Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Explorer or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

FFV Fuel (E-85) Capable Model

Special Service (Police, etc.) Package Upgrade

Two (2) Wheel Drive Drivetrain

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*  **MODEL YEAR 2021 OR NEWER: SMALL/MID-SIZE CROSSOVER VEHICLE;**  **AWD** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  106 inches to 115 inches |
| **ENGINE:**  1.5 liter minimum |
| 3 cylinder minimum |
| **TRANSMISSION:**  Automatic |
| **DRIVETRAIN:**  All Wheel Drive |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire Tools and Compact Jack Included |
| **SEATS:**  Cloth |
| Manufacturer’s Standard Front Seats |
| Manufacturer’s Standard Rear Bench Type Seat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless  Entry Transmitters |
| **If model proposed is flex fuel (E-85 capable):**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Escape*,* Chevrolet Equinox or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

Front Wheel Drive (FWD) Drivetrain

FFV Fuel (E-85) Capable Model

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*  **MODEL YEAR 2021 OR NEWER: STANDARD/FULL-SIZE CROSSOVER VEHICLE;**  **AWD; 6-CYLINDER** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  116 inches to 122 inches |
| **ENGINE:**  3.3liter minimum |
| 6 cylinder minimum |
| **TRANSMISSION:**  Automatic |
| **DRIVETRAIN:**  All Wheel Drive |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire Tools and Compact Jack Included |
| **SEATS:**  Cloth |
| Manufacturer’s Standard Front Seats |
| 2nd Row Split Bench Seat |
| 3rd Row Split Bench Seat – Ability to Fold Flat |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |
| **If model proposed is flex fuel (E-85 capable):**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Traverse, Dodge Durango or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitters

Bluetooth Connectivity

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

Front Wheel Drive (FWD) Drivetrain

FFV Fuel (E-85) Capable Model

Off-Road Package

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS*  **MODEL YEAR 2021 OR NEWER: SEVEN (7) PASSENGER, MINI-VAN; ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  120 inch minimum |
| **OVERALL LENGTH:**  189 inch minimum |
| **ENGINE:**  2.0 liter minimum |
| 4 cylinder minimum |
| **Flex-Fuel (E-85 and gasoline)** |
| **TRANSMISSION:**  4 speed or Constantly Variable Transmission (CVT) minimum |
| Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| Front and rear |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Cloth Seats |
| 2nd and 3rd Row Seating must be “Fold Flat” Type Seating |
| Full Length Carpeting |
| Automatic Speed Control |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Daytime Running Lamps |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or KeyFOBS with Remote Keyless Entry Transmitters |
| FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is  FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Transit Connect Passenger or other make/model equivalent** |

Possible options to be requested by agency:

Privacy Glass

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Heavy Duty Suspension

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS*  **MODEL YEAR 2021 OR NEWER: SEVEN (7) PASSENGER, MINI-VAN; REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  120 inch minimum |
| **OVERALL LENGTH:**  189 inch minimum |
| **ENGINE:**  2.0 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**  4 speed or Constantly Variable Transmission (CVT) minimum |
| Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare/Inflatable SpareAcceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| Front and rear |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Cloth Seats |
| 2nd and 3rd Row Seating must be “Fold Flat” Type Seating |
| Full Length Carpeting |
| Automatic Speed Control |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Daytime Running Lamps |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or KeyFOBS with Remote Keyless  Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chrysler Voyager or other make/model equivalent** |

Possible options to be requested by agency:

Privacy Glass

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Heavy Duty Suspension

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS*  **MODEL YEAR 2021 OR NEWER: TWELVE (12) PASSENGER FULL-SIZE VAN** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  135 to 148 inches |
| **OVERALL LENGTH:**  216 to 238 inches |
| **ENGINE:**  3.5 L minimum |
| 6 cylinder minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  8,500 lbs. minimum |
| **PAYLOAD:**  Manufacturer’s Standard |
| **TRANSMISSION:**  Automatic |
| 4 Speed minimum |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Front and Rear Air Conditioning and Heating Required |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Roll Stability Control |
| Manufacturer’s Standard Front and Rear Seats |
| Manufacturer’s Standard Flooring |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Power Windows |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is  FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Transit Passenger Wagon, Chevrolet Express Passenger or other make/model equivalent** |

Possible options to be requested by agency:

Privacy Glass

3rd Set of Keys or Key FOBS with remote keyless entry transmitters

Bluetooth Connectivity

Blind Spot Warning Feature

Backup Camera

Door: Sliding Side

Towing Package: Manufacturer’s Standard

Engine: Larger Size

Optional Rear Axle Ratio

GVWR Upgrade

FFV Fuel (E-85) Capable Model

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS*  **MODEL YEAR 2021 OR NEWER: FIFTEEN (15) PASSENGER FULL-SIZE VAN** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  138 to 155 inches |
| **OVERALL LENGTH:**  236 to 245 inches |
| **ENGINE:**  3.5 L minimum |
| 6 cylinder minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  8,500 lbs. minimum |
| **PAYLOAD:**  Manufacturer’s Standard |
| **TRANSMISSION:**  Automatic |
| 4 Speed minimum |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Front and Rear Air Conditioning and Heating Required |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding  NHTSA requirements |
| Manufacturer’s Standard Roll Stability Control |
| Manufacturer’s Standard Front and Rear Seats |
| Manufacturer’s Standard Flooring |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Power Windows |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is  FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Transit Passenger Wagon, Chevrolet Express Passenger Extended Wheelbase or other make/model equivalent** |

Possible options to be requested by agency:

Privacy Glass

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

Backup Camera

Door: Sliding Side

Towing Package: Manufacturer’s Standard

Engine: Larger Size

Optional Rear Axle Ratio

GVWR Upgrade

FFV Fuel (E-85) Capable Model

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS*  **MODEL YEAR 2021 OR NEWER: FIFTEEN (15) PASSENGER FULL-SIZE VAN, DRW** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  147.6 inches |
| **OVERALL LENGTH:**  263.9 inches |
| **OVERALL HEIGHT:**  107.7inches |
| **ENGINE:**  3.5 L Turbo minimum |
| 6 cylinder minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard |
| **REAR AXLE:**  Dual-rear wheel |
| **TRANSMISSION:**  Automatic |
| 10 Speed minimum |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Seven (7) |
| Manufacturer’s Standard All Season |
| Full Size Spare required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Front and Rear Air Conditioning and Heating Required |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Roll Stability Control |
| Manufacturer’s Standard Front and Rear Seats |
| Manufacturer’s Standard Flooring |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Power Windows |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless  Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Transit Passenger Wagon DRW or equivalent** |

Possible options to be requested by agency:

Privacy Glass

Fixed Glass

Bluetooth Connectivity

Blind Spot Warning Feature

All Wheel Drive

Side Door: Swing Out

Towing Package: Manufacturer’s Standard

Engine: Smaller Size

Reverse Sensing System

Reverse Alarm

Power Folding Heated Mirrors with Turn signals

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: FULL SIZE SPORT UTILITY VEHICLE;**  **4X4, RERGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  120 inches minimum |
| **ENGINE:**  3.5liter minimum |
| 6cylinder minimum |
| **TRANSMISSION:**  10-Speed minimum |
| Automatic |
| **DRIVETRAIN:**  Four (4) Wheel Drive |
| **TRANSFER CASE:**  Manufacturer’s Standard for Specific Transmission |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Backup Camera |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Cloth Front and Rear Seats |
| Manufacturer’s Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote  Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Tahoe or other make/model equivalent** |

Possible options to be requested by agency:

Towing Package: Manufacturer’s Standard

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Blind Spot Warning Feature

Console Full Floor (mini console not acceptable)

Fog Lights

Privacy Glass

Off-Road Package

Special Service (Police, etc.) Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: SMALL SPORT UTILITY VEHICLE;**  **PLUG-IN HYBRID** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  103.8 to 106.7 inches |
| **ENGINE:**  1.4 liter minimum |
| 4 cylinder maximum |
| **TRANSMISSION:**  4 speed minimum |
| Automatic |
| **DRIVETRAIN:**  Two (2) Wheel Drive |
| **BATTERY:**  Lithium-Ion Battery Pack System |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **GROUND CLEARANCE:**  7.5 inches minimum |
| **DOORS:**  Four (4) |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **TIRES:**  Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating | |
| **RADIO:**  Manufacturer’s Standard | |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements | |
| Automatic Speed Control | |
| Daytime Running Lamps | |
| Tilt Wheel | |
| Electric Rear Window Defroster | |
| Power Windows (front and back) | |
| Power Door Locks | |
| Exterior Mirrors with interior remote adjustment | |
| Manufacturer’s Standard Cloth Front and Rear Seats | |
| Manufacturer Standard Floor Mats (front and rear) | |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters | |
| **EXTERIOR COLORS:**  Manufacturer’s Standard | |
| **REFERENCE MODELS: Ford Escape Plug-In Hybrid or other make/model equivalent** | |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Bluetooth Connectivity

Blind Spot Warning Feature

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES*  **MODEL YEAR 2021 OR NEWER: ELECTRIC SPORT UTILITY VEHICLE** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:**  115 to 119 inches |
| **DRIVETRAIN:**  Two (2) Wheel Drive |
| **BATTERY:**  Lithium-Ion Battery Pack System |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **DOORS:**  Four (4) |
| **TIRES:**  Four (4) |
| Manufacturer’s Standard All Season |
| Tire Inflation and Sealant Kit OR Tire Tools and Compact Jack must be included |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lamps |
| Tilt Wheel |
| Electric Rear Window Defroster |
| Power Windows (front and back) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Manufacturer’s Standard Cloth Front and Rear Seats |
| Manufacturer Standard Floor Mats (front and rear) |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Mach-E or equivalent** |

Possible options to be requested by agency:

3rd Set of Keys or Key FOBS with remote keyless entry transmitter

Extended Range Battery

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UNSPSC Code*: 25101503: AUTOMOBILES OR CARS*

**MISCELLANEOUS OPTIONS / FEATURES**

1 TOTL

Line item shall be used for the purchase of miscellaneous vehicle options/features not specified herein. Prior to issuing a purchase order, the state agency shall contact the contractor to obtain the price for the option required.