**ATTACHMENT 2 – LIGHT DUTY TRUCKS AND WORK VANS**

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: SMALL/MID-SIZE TRUCK; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 126.8 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**2.3 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length 6’ 2” (variance +/- 2 inches) |
| Wide Type |
| **CAB:**Extended Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Dual Rear Seats |
| Two (2) Sets of Keys or Key FOBS  |

|  |
| --- |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Colorado , Ford Ranger or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Cloth Front and Rear Bench Seat

 Cloth Front Bucket Seats without Center Console

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Remove Center Console

Integrated Brake Controller

 Fog Lights

 Optional Rear Axle Ratio

Crew Cab

 Long Bed

 Short Bed (Crew Cab Only)

 Engine: Larger Size

Engine: Diesel

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: SMALL/MID-SIZE TRUCK; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 126.8 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**2.3 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length 6’ 2” (variance +/- 2 inches) |
| Wide Type |
| **CAB:**Extended Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Dual Rear Seats |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Colorado, Ford Ranger or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Cloth Front and Rear Bench Seat

 Cloth Front Bucket Seats Without Center Console

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless

 Entry with two (2) transmitters

 Remove Center Console

Integrated Brake Controller

 Fog Lights

 Optional Rear Axle Ratio

Crew Cab

 Long Bed

 Short Bed (Crew Cab Only)

 Engine: Larger Size

Engine: Diesel

 FFV Fuel (E-85) Capable Model

Off Road Tires

 Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X2; REGULAR CAB;** **ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 119 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,000 lbs. minimum  |
| **ENGINE:**3.3 liter minimum |
| 6 cylinder  |
| **Flexible Fuel Capable** |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length - 6 feet minimum |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |

|  |
| --- |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 1500 FFV, Ford F150 FFV or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Optional Rear Axle Ratio

 Long Bed

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X2; EXTENDED CAB;** **ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 140 inch minimum  |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,100 lbs. minimum  |
| **ENGINE:**3.3 liter minimum |
| 6 cylinder  |
| **Flexible Fuel Capable** |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 6 feet minimum |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 1500 FFV, Ford F150 FFV or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Crew Cab

Optional Rear Axle Ratio

 Long Bed

 Short Bed (Crew Cab only)

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

 Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X4; REGULAR CAB;** **ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 119 minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,050 lbs. minimum  |
| **ENGINE:**3.3 liter minimum |
| 6 cylinder minimum |
| **Flexible Fuel Capable** |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 6 feet minimum |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 1500 FFV, Ford F150 FFV or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Fog Lights

 Off Road Tires

Optional Rear Axle Ratio

 Long Bed

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X4; EXTENDED CAB;** **ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 140 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,300 lbs. minimum  |
| **ENGINE:**3.3 liter minimum |
| 6 cylinder minimum |
| **Flexible Fuel Capable** |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 6 feet minimum |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 1500 FFV, Ford F150 FFV or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Off Road Tires

 Crew Cab

Optional Rear Axle Ratio

 Long Bed

 Short Bed (Crew Cab only)

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X2; REGULAR CAB; REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 119 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,000 lbs. minimum  |
| **ENGINE:**2.7 liter minimum |
| 4 cylinder, minimum  |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length - 6’ 4” minimum |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 1500, Ford F150, Dodge Ram 1500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Optional Rear Axle Ratio

 Long Bed

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X2; EXTENDED CAB; REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 140 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,100 lbs. minimum  |
| **ENGINE:**2.7 liter minimum |
| 4 cylinder, minimum  |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 6 feet minimum |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 1500, Ford F150, Dodge Ram 1500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Crew Cab

 Optional Rear Axle Ratio

 Long Bed

 Short Bed (Crew Cab only)

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

 Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X4; REGULAR CAB; REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 119 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,050 lbs. minimum  |
| **ENGINE:**2.7 liter minimum |
| 4cylinder minimum |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length 6’ 4” minimum |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 1500, Ford F150, Dodge Ram 1500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Off Road Tires

Optional Rear Axle Ratio

 Long Bed

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X4; EXTENDED CAB; REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 140 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 6,300 lbs. minimum  |
| **ENGINE:**2.7 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 6 feet minimum |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 1500, Ford F150, Dodge Ram 1500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Off Road Tires

 Crew Cab

Optional Rear Axle Ratio

 Long Bed

 Short Bed (Crew Cab only)

 Engine: Larger Size

 Engine: Smaller Size

 GVWR/Payload Upgrade

 Towing Package: Manufacturer’s Standard

 Special Service Package Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: 3/4 TON TRUCK; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 132 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 8,600 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 8 feet (variance +/- 6 inches) |
| Wide Type |

|  |
| --- |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5), Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 2500, Ford F250, Dodge Ram 2500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats

 Front: High Back Cloth Bucket Seats without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Trailer Brake Controller

Optional Rear Axle Ratio

 Short Bed

 Engine: Diesel

 FFV Fuel (E-85) Capable Model

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 or newer: 3/4 TON TRUCK; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 144 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 8,800 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 6’ 6” (variance +/- 3 inches) |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5), Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **Minimum Mandatory Specifications** |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 2500, Ford F250, Dodge Ram 2500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Trailer Brake Controller

Optional Rear Axle Ratio

 Long Bed

 Crew Cab

Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

Running Boards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: 3/4 TON TRUCK; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 133 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 8,600 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for specific transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 8 feet (variance +/- 6 inches) |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 2500, Ford F250, Dodge Ram 2500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Off Road Tires

Optional Rear Axle Ratio

 Short Bed

 Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

Running Boards

**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: 3/4 TON TRUCK; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 141 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 8,800 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for specific transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 6’ 6” (variance +/- 3 inches) |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 2500, Ford F250, Dodge Ram 2500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Off Road Tires

Optional Rear Axle Ratio

 Long Bed

 Crew Cab

Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Running Boards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: ONE TON TRUCK; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 132 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 9,900 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 8 feet (variance +/- 6 inches) |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5), Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 3500, Ford F350, Dodge Ram 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats

 Front: High Back Cloth Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Optional Rear Axle Ratio

 Short Bed

 Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Dual Rear Wheel:

Running Boards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: ONE TON TRUCK; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 144 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 10,000 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **BED:**Standard Bed |
| Length – 6’ 3” minimum |
| Wide Type |

|  |
| --- |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:** Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Chevrolet Silverado 3500, Ford F350, Dodge Ram 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats Without Center Console

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Optional Rear Axle Ratio

 Long Bed

 Crew Cab

Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Dual Rear Wheel:

Running Boards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: ONE TON TRUCK; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 133 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 9,900 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for specific transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 8 feet (variance +/- 6 inches) |
| Wide Type |
| **CAB:**Regular Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 3500, Ford F350, Dodge Ram 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Off Road Tires

Optional Rear Axle Ratio

 Short Bed

 Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Dual Rear Wheel

Running Boards

**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: ONE TON TRUCK; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 141 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 10,400 lbs. minimum  |
| **ENGINE:**6.2 liter minimum |
| 8 cylinder  |
| Gasoline |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for specific transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length – 6’ 3” minimum |
| Wide Type |
| **CAB:**Extended Cab minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet Silverado 3500, Ford F350, Dodge Ram 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Blind Spot Warning Feature

 Trailer Tow Mirrors

 Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Transmission: Manual

 Fog Lights

 Trailer Brake Controller

Off Road Tires

Optional Rear Axle Ratio

 Long Bed

 Crew Cab

Engine: Diesel

 Engine: Larger Gas

GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

 Dual Rear Wheel:

Running Boards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS* **MODEL YEAR 2021 OR NEWER: CARGO MINI-VAN, REGULAR FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 115 inch minimum  |
| **OVERALL LENGTH:**186 inch minimum |
| **ENGINE:**Manufacturer’s Standard 4 Cylinder |
| 2.0 L minimum |
| **TRANSMISSION:**Manufacturer’s Standard Constantly Variable Transmission (CVT) or Automatic 6 Speed minimum  |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Front Seats |
| Rear Vinyl/Rubber Flooring |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Power Windows (front) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitter |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Dodge Ram Promaster City, Ford Transit Connect or other make/model equivalent** |

 Possible options to be requested by agency:

Electric Rear Window Defroster

 3rd Set of Keys or Key FOBS with remote keyless entry transmitter

 Bluetooth Connectivity

 Blind Spot Warning Feature

 Heavy Duty Suspension

 Backup Camera

 Door: Sliding Side

 Second Row Driver and Passenger Door Window

Rear Door Windows

 Driver/Passenger Protection Panel

 Rear Heating and Air Conditioning

 FFV Fuel (E-85) Capable Model

Cargo Van Group Options

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS* **MODEL YEAR 2021 OR NEWER: CARGO MINI-VAN, ALTERNATIVE FUEL** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 115 inch minimum  |
| **OVERALL LENGTH:**186 inch minimum |
| **ENGINE:**Manufacturer’s Standard 4 Cylinder |
| 2.0 L minimum, **Flex Fuel Capable** |
| **TRANSMISSION:**Manufacturer’s Standard Constantly Variable Transmission (CVT) or Automatic 6 Speed minimum  |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Front Seats |
| Rear Vinyl/Rubber Flooring |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Power Windows (front) |
| Power Door Locks |
| Exterior Mirrors with interior remote adjustment |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitter |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Transit Connect or other make/model equivalent** |

 Possible options to be requested by agency:

Electric Rear Window Defroster

 3rd Set of Keys or Key FOBS with remote keyless entry transmitter

 Bluetooth Connectivity

 Blind Spot Warning Feature

 Heavy Duty Suspension

 Backup Camera

 Door: Sliding Side

 Second Row Driver and Passenger Door Window

Rear Door Windows

 Driver/Passenger Protection Panel

 Rear Heating and Air Conditioning

 FFV Fuel (E-85) Capable Model

Cargo Van Group Options

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS* **MODEL YEAR 2021 OR NEWER: FULL-SIZE CARGO VAN** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 129.9 inches minimum  |
| **OVERALL LENGTH:**213 inches minimum |
| **ENGINE:**3.5 L minimum |
| 6 or 8 cylinder |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**8,500 lbs. minimum |
| **PAYLOAD:**Manufacturer’s Standard |
| **TRANSMISSION:**Automatic  |
| 4 Speed minimum |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Front Vinyl Seats |
| Manufacturer’s Standard Roll Stability Control |
| Front – Black Rubberized/Vinyl Floor Coverings |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
|  **REFERENCE MODELS: Ford Transit Cargo, Chevrolet Express Cargo, Dodge Ram Promaster or other make/model equivalent** |

 Possible options to be requested by agency:

Power Windows, Power Door Locks and Power Exterior Mirrors

 3rd Set of Keys or Key FOBS with remote keyless entry transmitter

 Bluetooth Connectivity

 Blind Spot Warning Feature

 Backup Camera

 Door: Sliding Side

 Towing Package: Manufacturer’s Standard

 Heavy Duty Suspension

 Driver/Passenger Protection Panel

 Rear Door Windows

 Passenger Side Door Glass

Rear Air Conditioning and Heating

Rear Cargo Liner or Rubberized/Vinyl Floor Covering

Engine: Larger Size

 Engine: Diesel

 Extended Length

Optional Rear Axle Ratio

 GVWR Upgrade

 FFV Fuel (E-85) Capable Model

 Cargo Van Group Options

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505: MINI VANS OR VANS* **MODEL YEAR 2021 OR NEWER: FULL-SIZE ELECTRIC CARGO VAN** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 129.9 inches minimum  |
| **OVERALL LENGTH:**213 inches minimum |
| **BATTERY:**Lithium-Ion Battery Pack System |
| **PAYLOAD:**Manufacturer’s Standard |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Manufacturer’s Standard Front Vinyl Seats |
| Manufacturer’s Standard Roll Stability Control |
| Front – Black Rubberized/Vinyl Floor Coverings |
| Automatic Speed Control |
| Tilt Wheel |
| Daytime Running Lamps |
| Two (2) Sets of Keys or Key FOBS with Remote Keyless Entry Transmitters  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford E-Transit Cargo or other make/model equivalent** |

 Possible options to be requested by agency:

Power Windows, Power Door Locks and Power Exterior Mirrors

 3rd Set of Keys or Key FOBS with remote keyless entry transmitter

 Bluetooth Connectivity

 Blind Spot Warning Feature

 Backup Camera

 Door: Sliding Side

 Towing Package: Manufacturer’s Standard

 Driver/Passenger Protection Panel

 Rear Door Windows

 Passenger Side Door Glass

Rear Air Conditioning and Heating

Rear Cargo Liner or Rubberized/Vinyl Floor Covering

 Extended Length

 GVWR Upgrade

 Cargo Van Group Options

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: SMALL TRUCK; ALL-WHEEL DRIVE; CREWCAB** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 121 inches minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**2.0 liter minimum |
| 4 cylinder minimum |
| **TRANSMISSION:**4 speed minimum  |
| Automatic |
| **TRANSFER CASE:**Manufacturer’s Standard for Specific Transmission |
| **AUTO LOCKING HUBS:**Manufacturer’s Standard |
| **BED:**Standard Bed |
| Length 4’ 6” (variance +/- 2 inches) |
| Wide Type |
| **CAB:**Crew Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Compact Spare Acceptable for 5th tire |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Seats |
| Two (2) Sets of Keys or Key FOBS  |
| Power Windows and Door Locks |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford Maverick or other make/model equivalent** |

 Possible options to be requested by agency:

Trailer Tow Package

3rd Set of Keys or Key FOBS

 Manual Rear Sliding Window

Blind Spot Warning Feature

 Hybrid option

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101507: LIGHT TRUCKS OR SPORT UTILITY VEHICLES* **MODEL YEAR 2021 OR NEWER: HALF TON TRUCK; 4X4; CREW CAB; ELECTRIC** |
| **Minimum Mandatory Specifications** |
| **WHEELBASE:** 145 inch minimum |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer Standard  |
| **BATTERY:**Lithium-Ion Battery Pack System |
| **BED:**Standard Bed |
| Length – 5.5 feet minimum |
| Wide Type |
| **CAB:**Crew Cab |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power  |
| **TIRES:**Five (5) |
| Manufacturer’s Standard All Season |
| Full Size Spare Required |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Daytime Running Lights |
| Automatic Speed Control |
| Tilt Wheel |
| Painted or Chrome Rear Step Type Bumper |
| Cloth Front and Rear Bench Type Seat |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F150 Lightning or other make/model equivalent** |

 Possible options to be requested by agency:

3rd Set of Keys or Key FOBS

 Trailer Tow Mirrors

 Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Fog Lights

 Off Road Tires

 GVWR/Payload Upgrade

Towing Package: Manufacturer’s Standard

Extended Range Battery

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UNSPSC Code*: 25101507: LIGHT TRUCK OR SUV*  1 TOTL

 **MISCELLANEOUS OPTIONS / FEATURES**

Line item shall be used for the purchase of miscellaneous vehicle options/features not specified herein. Prior to issuing a purchase order, the state agency shall contact the contractor to obtain the price for the option required.