**ATTACHMENT 3 – MEDIUM DUTY TRUCKS AND CARGO VANS**

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60”  |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60”  |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

 84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |

|  |
| --- |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

 Towing Package: Manufacturer’s Standard

 84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60”  |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |

|  |
| --- |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

 84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

 84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

 Towing Package: Manufacturer’s Standard

 84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |

|  |
| --- |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

 Towing Package: Manufacturer’s Standard

 84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

 3rd Set of Keys or Key FOBS

 Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 21,900 lbs. minimum  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **If model proposed is flex fuel:**FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F600 or other make/model equivalent** |

 Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

 Cloth Front Seat

 Cloth Front Bucket Seats

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 Running Boards

 Fog Lights

 Optional Rear Axle Ratio

 Engine: Gas

 FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

Extended Cab

Crew Cab

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 25,500 lbs.  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**632,000 in.-lbs. Resisting Bending Moment |

|  |
| --- |
| **BRAKES:**Hydraulic with Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Tilt Wheel |
| Cruise Control |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

 Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

120” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 25,500 lbs.  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**632,000 in.-lbs. Resisting Bending Moment |

|  |
| --- |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Cruise Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

 Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** Manufacturer’s Standard for Model Proposed  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**632,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**Hydraulic Four-Wheel Antilock Brakes (ABS) |

|  |
| --- |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Automatic Speed Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

 Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 31,000 lbs.  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**Hydraulic with Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |

|  |
| --- |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Tilt Wheel |
| Cruise Control |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

 Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

120” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 31,000 lbs.  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |

|  |
| --- |
| **REAR AXLE RATIO:**Manufacturer’s Standard |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Cruise Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

 Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS* **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):** 31,000 lbs.  |
| **ENGINE:**6.6 liter minimum; diesel |
| **TRANSMISSION:**Automatic |
| **FRAME:**1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**Hydraulic Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**Power Steering |
| **REAR AXLE RATIO:**Manufacturer’s Standard |

|  |
| --- |
| **TIRES:**Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**Manufacturer’s Standard  |
| **OTHER EQUIPMENT & FEATURES:**Automatic Speed Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS  |
| **EXTERIOR COLORS:**Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

Possible options to be requested by agency:

 Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

 108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UNSPSC Code*: 25181602: TRUCK CHASSIS*  1 TOTL

**MANUFACTURER MISCELLANEOUS OPTIONS / FEATURES**

Line item shall be used for the purchase of miscellaneous vehicle options/features not specified herein. Prior to issuing a purchase order, the state agency shall contact the contractor to obtain the price for the option required.