**ATTACHMENT 3 – MEDIUM DUTY TRUCKS AND CARGO VANS**

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |

|  |
| --- |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to Axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: ONE TON CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 3500 , Ford F350, Dodge 3500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |

|  |
| --- |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 4 CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 4500 , Ford F450, Dodge 4500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |

|  |
| --- |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 5500 , Ford F550, Dodge 5500 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 5 CHASSIS CAB DRW; 4X4; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  60” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  21,900 lbs. minimum |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), plus spare |
| Manufacturer’s Standard All Season |
| Tire tools and jack required |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Air Bags – Manufacturer Standard meeting or exceeding NHTSA requirements |
| Automatic Speed Control |
| Daytime Running Lights |
| Tilt Wheel |
| Factory Trailer Brake Controller |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **If model proposed is flex fuel:**  FFV (E-85) Fuel Identifier – must have distinguishing identifier in the fuel fill port which indicates vehicle is FFV (E-85) – i.e. yellow fuel cap, yellow E-85 sticker) |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F600 or other make/model equivalent** |

Possible options to be requested by agency:

Axle, Rear: Limited Slip

3rd Set of Keys or Key FOBS

Bluetooth Connectivity

Upfitter Interface Module

Cloth Front Seat

Cloth Front Bucket Seats

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

Running Boards

Fog Lights

Optional Rear Axle Ratio

Engine: Gas

FFV Fuel (E-85) Capable Model

Towing Package: Manufacturer’s Standard

84” Cab to axle

108” Cab to axle

Block Heater

High Capacity Trailer Tow

Rear Backup Camera Preparation Pkg

Payload Upgrade

Extended Cab

Crew Cab

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  25,500 lbs. |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  632,000 in.-lbs. Resisting Bending Moment |

|  |
| --- |
| **BRAKES:**  Hydraulic with Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Tilt Wheel |
| Cruise Control |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

120” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  25,500 lbs. |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  632,000 in.-lbs. Resisting Bending Moment |

|  |
| --- |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Cruise Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 6 CHASSIS CAB DRW; 4X2; CREW CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  Manufacturer’s Standard for Model Proposed |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  632,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**  Hydraulic Four-Wheel Antilock Brakes (ABS) |

|  |
| --- |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Automatic Speed Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Chevrolet 6500 , Ford F650 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; REGULAR CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  31,000 lbs. |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**  Hydraulic with Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |

|  |
| --- |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Tilt Wheel |
| Cruise Control |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

120” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; EXTENDED CAB** |
| **Minimum Mandatory Specifications** |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  31,000 lbs. |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**  Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |

|  |
| --- |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Cruise Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |  |
| --- | --- |
| UNSPSC Code*: 25181602: TRUCK CHASSIS*  **MODEL YEAR 2021 OR NEWER: CLASS 7 CHASSIS CAB DRW; 4X2; CREW CAB** | |
| **Minimum Mandatory Specifications** | |
| **Cab to Axle:**  84” |
| **GROSS VEHICLE WEIGHT RATING (GVWR):**  31,000 lbs. |
| **ENGINE:**  6.6 liter minimum; diesel |
| **TRANSMISSION:**  Automatic |
| **FRAME:**  1,200,000 in.-lbs. Resisting Bending Moment |
| **BRAKES:**  Hydraulic Four-Wheel Antilock Brakes (ABS) |
| **STEERING:**  Power Steering |
| **REAR AXLE RATIO:**  Manufacturer’s Standard |

|  |
| --- |
| **TIRES:**  Six (6), 11R22.5 |
| Manufacturer’s Standard Steer Tires and Traction Tread Rear |
| **AIR CONDITIONING & HEATING:**  Manufacturer’s Standard Air Conditioning and Heating |
| **RADIO:**  Manufacturer’s Standard |
| **OTHER EQUIPMENT & FEATURES:**  Automatic Speed Control |
| Tilt Wheel |
| Vinyl Seats and flooring |
| Two (2) Sets of Keys or Key FOBS |
| **EXTERIOR COLORS:**  Manufacturer’s Standard |
| **REFERENCE MODELS: Ford F750 or other make/model equivalent** |

Possible options to be requested by agency:

Power Windows, Power Door Locks, Power Exterior Mirrors & Remote Keyless Entry with two (2) transmitters

108” Cab to axle

Gasoline engine

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UNSPSC Code*: 25181602: TRUCK CHASSIS*  1 TOTL

**MANUFACTURER MISCELLANEOUS OPTIONS / FEATURES**

Line item shall be used for the purchase of miscellaneous vehicle options/features not specified herein. Prior to issuing a purchase order, the state agency shall contact the contractor to obtain the price for the option required.