**ATTACHMENT 4 – PATROL VEHICLES**

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: CHEVROLET TAHOE 2WD 9C1 PURSUIT UTILITY VEHICLE** |
| **Mandatory Specifications** |
| **FRONT SEATS:**  Heavy duty cloth 40/20/40 split bench style seating **without** center 20% section; Center section must be deleted |
| Power driver and front passenger seat adjusters |
| **REAR SEAT:**  Third row seating deleted |
| **FLOOR COVERING:**  Full, color keyed carpeting |
| **FLOOR MATS:**  Manufacturer’s first and second row color keyed carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **KEYS:**  Two (2) keyless entry key Fobs |
| **SPOTLIGHT PROVISION/SPOTLIGHT, LEFT HAND:**  Left (driver side) factory spotlight provision |
| 6” LED spotlight installed |
| **AUXILIARY DOME LAMP:**  Factory installed red/white overhead high intensity auxiliary dome lamp |
| The auxiliary lamp is wired independently from the standard dome lamp |
| **WIRING:**  Grill lamp and siren speaker wiring for connection to agency-furnished equipment required |
| Horn/siren wiring circuit for connection of agency-furnished switch required |
| Center Console wiring harness with auxiliary power outlet kit is required |
| **FLASHER SYSTEM:**  Headlamps and Trail Lamps, Tail Lamps alternate flashing red/white |
| **RADIO SUPPRESSION PACKAGE** |
| **FLEET FREE MAINTENANCE CREDIT:**  Credit in lieu of free oil changes, tire rotations and inspections during the first 24 months/24,000 miles |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| **MANDATORY MODEL: Chevrolet Tahoe 2WD 9C1 Pursuit Utility Vehicle** |

Possible options to be requested by agency:

4WD 9C1 Pursuit Option

Complete 40/20/40 cloth front bench seating

Four (4) extra key

Black vinyl floor covering

Remove radio suppression system

17” x 8” machined aluminum wheels

Molded Splash Guards

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: CHEVROLET TAHOE 4WD SPECIAL SERVICE VEHICLE** |
| **Mandatory Specifications** |
| **FLOOR COVERING:**  Full, color keyed carpeting |
| **FLOOR MATS:**  Manufacturer’s first and second row color keyed carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **KEYS:**  Two (2) keyless entry key fobs |
| **AUXILIARY DOME LAMP:**  Factory installed red/white overhead high intensity auxiliary dome lamp |
| The auxiliary lamp is wired independently from the standard dome lamp |
| **WIRING:**  Grill lamp and siren speaker wiring for connection to agency-furnished equipment required |
| Horn/siren wiring circuit for connection of agency-furnished switch required |
| **FLASHER SYSTEM:**  Headlamps and Trail Lamps, Tail Lamps alternate flashing red/white |
| **RADIO SUPPRESSION PACKAGE** |
| **FLEET FREE MAINTENANCE CREDIT:**  Credit in lieu of free oil changes, tire rotations and inspections during the first 24 months/24,000 miles |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Chevrolet Tahoe 4WD Special Service Vehicle** |

Possible options to be requested by agency:

Four (4) extra key Keyless Entry Transmitters

Black vinyl floor covering

Molded Splash Guards

Remove radio suppression system

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: DODGE CHARGER PURSUIT ALL-WHEEL DRIVE SEDAN** |
| **Mandatory Specifications** |
| **ENGINE:**  3.6 liter V6 |
| **ALL WHEEL DRIVE** |
| **TIRES:**  Five (four tires plus spare) |
| Goodyear P245/55R18 “W” Speed Rated |
| Includes full size spare |
| **WHEEL COVERS:**  Manufacturer’s 18” full wheel covers required |
| **SPARE TIRE RELOCATION BRACKET:**  Manufacturer’s spare tire relocation bracket required |
| **FRONT SEATS:**  Heavy duty bucket seats |
| Reinforced for increased support |
| Covered with heavy duty cloth fabric |
| No center console |
| Power adjusting driver seat required |
| **KEYS:**  Four (4) keyless entry Fobs |
| **REAR SEAT:**  Heavy duty cloth fabric rear bench seat |
| **FLOOR COVERING:**  Full carpeting, both front and rear |
| **FLOOR MATS:**  Manufacturer’s carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **SPOTLIGHT PROVISION/SPOTLIGHT, LEFT HAND:**  Left (driver side) factory spotlight provision |
| 6” spotlight installed |
| **AUXILIARY DOME LAMP:**  Factory installed overhead high intensity red/white auxiliary dome lamp |
| Wired and switched independently from standard dome lamp |
| **POLICE EQUIPMENT MOUNTING BRACKET:**  Factory installed police equipment mounting bracket located between the front seats required |
| **FLEET SAFETY GROUP:**  Includes blind spot monitoring, power adjusting, heated, manual folding pursuit mirrors |
| Exterior mirrors with heating element |
| **PARK SENSE**:  Rear park assist system |
| **SECURE PARK:**  Allows driver to leave the engine running and prevents unauthorized vehicle use |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Dodge Charger Pursuit All-Wheel Drive Sedan** |

Possible options to be requested by agency:

5.7 liter V-8 Rear Wheel Drive

12.1 inch Integrated Display Package

Additional Key FOBS

Vinyl Floor Covering In Lieu of Carpet

Vinyl Rear Bench Seat in Lieu of Cloth

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: DODGE DURANGO PURSUIT ALL-WHEEL DRIVE SPORT UTILITY VEHICLE** |
| **Mandatory Specifications** |
| **ENGINE:**  5.7 liter V8 |
| **ALL WHEEL DRIVE** |
| Two speed, electronically shifted transfer case |
| **TIRES:**  Four (4) |
| P255/60R18 V rated |
| Spare tire – P255/60R18 V rated |
| **WHEELS:**  Steel wheels with chrome center cap |
| Includes full size spare |
| **SINGLE KEY LOCKING SYSTEM:**  Single key system for ignition, door and lift gate |
| Each vehicle keyed differently |
| Factory installed keyless entry system with minimum of four 4) keyless entry key fobs |
| **FRONT SEATS:**  Heavy duty cloth bucket seats with center console delete |
| Power adjusting driver seat required |
| **SECOND ROW SEATING:**  Heavy duty cloth fabric |
| 60/40 bench seat |
| **THIRD ROW SEATING:**  None |
| **FLOOR COVERING:**  Full carpeting, both front and rear |
| **FLOOR MATS:**  Manufacturer’s carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **AUXILIARY DOME LAMP:**  Factory installed overhead high intensity red/white auxiliary dome lamp in passenger and cargo area |
| Wired and switched independently from standard dome lamp |
| **TOW PACKAGE:**  Factory installed tow package with class 4 receiver hitch  and trailer wiring. Inlcudes on demand 2 speed transfer case. |
| **SKID PLATE GROUP:**  Skid plates for fuel tank, transfer case, front suspension and underbody |
| **SPOTLIGHT:**  Driver side spotlight installed, 6” LED |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Dodge Durango Pursuit All-Wheel Drive Sport Utility Vehicle** |

Possible options to be requested by agency:

3.6 liter V6 gasoline engine

Vinyl in lieu of carpet

Optional vinyl second row seat

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: DODGE DURANGO SPECIAL SERVICE PACKAGE REAR WHEEL DRIVE SPORT UTILITY VEHICLE** |
| **Mandatory Specifications** |
| **ENGINE:**  5.7 liter V8 |
| **REAR WHEEL DRIVE** |
| **TIRES:**  Five (four tires plus spare) |
| Manufacturer’s standard for make/model |
| Includes full size spare |
| **WHEELS:**  Five (5) |
| Manufacturer’s standard wheels |
| Includes full size spare |
| Steel spare wheel is acceptable |
| **FRONT SEATS:**  Heavy duty cloth bucket seats |
| Power adjusting driver seat required |
| **SECOND ROW SEATING:**  Heavy duty cloth fabric |
| 60/40 bench seat |
| **THIRD ROW SEATING:**  None |
| **FLOOR COVERING:**  Full carpeting, both front and rear |
| **FLOOR MATS:**  Manufacturer’s carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **AUXILIARY DOME LAMP:**  Factory installed overhead high intensity red/white auxiliary dome lamp |
| Wired and switched independently from standard dome lamp |
| **TOW PACKAGE:**  Factory installed tow package with class 4 receiver hitch |
| **BACKUP CAMERA:**  Manufacturer’s standard backup camera required |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Dodge Durango Special Service Package Rear Wheel Drive Sport Utility Vehicle** |

Possible options to be requested by agency:

3.6 liter V6 gasoline engine in lieu of 5.7 liter V8 engine

Driver Side Spotlight, 6” LED, Installed

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: FORD POLICE INTERCEPTOR UTILITY** |
| **Mandatory Specifications** |
| **ENGINE:**  3.3 liter V6 direct injection FFV engine |
| **ALL WHEEL DRIVE** |
| **WHEEL COVERS:**  Manufacturers full wheel covers required |
| **REMOTE KEYLESS ENTRY SYSTEM:**  Remote keyless entry system with minimum of four (4) keyless entry key FOBS |
| **OUTSIDE REAR VIEW MIRRORS:**  Left hand and right hand power adjusting |
| Heated required |
| **FRONT SEATS:**  No center console |
| **REAR SEAT:**  Heavy duty cloth fabric rear bench seat |
| **FLOOR COVERING:**  Full carpeting, first and second rows |
| **FLOOR MATS:**  Manufacturer’s carpeted mats required |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **SPOTLIGHT PROVISION/SPOTLIGHT, LEFT HAND:**  Left (driver side) factory spotlight provision |
| LED spotlight installed |
| **POLICE POWER PIGTAIL:**  Power pigtail harness required |
| **WIRING:**  Pre-wiring for grill LED lamp, siren and speaker |
| **COURTESY LAMP DISABLE:**  Courtesy lamp disabled when any door is opened |
| **AUXILIARY DOME LAMPS:**  Factory installed first row overhead red/white auxiliary dome lamp |
| Factory installed red/white overhead dome lamp in cargo area |
| **POLICE INTERCEPTOR HEADLAMP HOUSINGS:**  Includes LED wig-wag feature |
| Pre-drilled holes for side marker police use |
| Does not include LED installed lights |
| **TAIL LAMP HOUSING PREP PACKAGE:**  Factory installed tail lamp housing prep package  required |
| Does not include LED installed lights. |
| **GLOBAL LOCK/UNLOCK FEATURE:**  Door panel switches will lock/unlock all doors and rear lift gate |
| **REVERSE SENSING:**  Reverse sensing system required |
| **NOISE SUPPRESSION BONDS:**  Factory installed radio noise suppression bonding straps required |
| **POLICE ENGINE IDLE FEATURE:**  Allows driver to leave the engine running and prevents unauthorized vehicle use |
| **UNDERBODY DEFLECTOR PLATE:**  Engine and transmission shield |
| **OBD-II SPLIT CONNECTOR:**  Allows up to two devices to be connected to the vehicle OBD-II Port |
| **TRAILER TOW:**  Class III Trailer Tow Lighting Package (4-pin and 7-pin connectors and wiring) |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Ford Police Interceptor Utility** |

Possible options to be requested by agency:

3.3 liter Direct Injection Hybrid Engine

3.0 liter V6 EcoBoost turbocharged engine

Black vinyl floor covering

Auxiliary air conditioning

Standard wheel center caps in lieu of full wheel covers

18”painted aluminum wheels in lieu of standard steel wheels. Spare will remain steel

Second row grey vinyl seating in lieu of cloth

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: FORD F-150 POLICE RESPONDER SUPERCREW** |
| **Mandatory Specifications** |
| **ENGINE:**  3.5 liter V6 EcoBoost |
| Gasoline |
| **FOUR WHEEL DRIVE** |
| **BODY:**  Four (4) door SuperCrew cab with 5.5' box |
| **TRANSMISSION:**  Ten (10) speed |
| Automatic |
| Column mounted gear selector |
| **ALTERNATOR:**  Manufacturer’s Standard |
| **STEERING:**  Power assist rack & pinion |
| **STEERING WHEEL:**  Manufacturer’s Standard |
| Tilt required |
| **BRAKES:**  Four (4) wheel anti-lock disc brakes |
| Power booster |
| **TIRES:**  Five (four tires plus spare) |
| LT265/70R18C all-terrain |
| Includes full size spare |
| **WHEELS:**  Five (5), Includes full size spare |
| 18" heavy duty |
| **CRUISE CONTROL:**  Factory installed required |
| **SPEEDOMETER:**  Calibrated and certified for accuracy |
| **AIR CONDITIONING & HEATING:**  Factory installed air conditioning |
| Integral heater and defroster |
| **ELECTRIC REAR WINDOW DEFROSTER:**  Manufacturer installed rear window defroster required |
| Privacy Glass |
| **POLICE IDLE FEATURE:**  Required |
| **RADIO:**  Manufacturer’s Standard AM/FM |
| **BLUETOOTH:**  Factory installed Bluetooth hands-free device |
| **REAR VIEW CAMERA:**  Manufacturer’s standard required |
| **REVERSE SENSING:**  Manufacturer's reverse sensing system required |
| **POWER WINDOWS AND DOOR LOCKS:**  Manufacturer’s standard required |
| Rear power windows must be operable from rear seat as well as from the driver’s seat |
| System must include a rear window lockout switch controllable from the driver’s position |
| **SINGLE KEY LOCKING SYSTEM:**  Single key system with each vehicle keyed differently |
| Remote keyless entry system with minimum of four (4)  keyless entry key fobs |
| **OUTSIDE REAR VIEW MIRRORS:**  Manual-folding, ***manually telescoping*** power glass trailer tow mirrors with heat. ***(54Y)*** |
| **FRONT SEATS:**  Heavy duty bucket style seating |
| Covered with heavy duty cloth fabric |
| Center section delete. No center console. |
| 8-way power adjusting driver seat required |
| **SECOND ROW SEATING:**  Heavy duty vinyl second row bench seat |
| **AIR BAGS:**  Manufacturer’s Standard |
| **FLOOR COVERING:**  Vinyl floor covering |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **TRAILER TOW PACKAGE:**  Class IV hitch |
| 4-pin/7-pin wiring harness |
| Auxiliary transmission oil cooler |
| Engine oil cooler |
| **TRAILER BRAKE CONTROLLER WITH BACKUP ASSIST:**  Factory installed trailer brake controller |
| **BUMPERS**:  Chrome front and rear required |
| **FOG LAMPS:**  Required |
| **RUNNING BOARDS:**  Drivers and passenger factory installed black running boards |
| **COLORS:**  Standard production solid color exterior and standard interior trim color |
| Colors will be selected after award |
| **MANDATORY MODEL: Ford F-150 Police Responder** |

Possible options to be requested by agency:

Delete chrome bumpers, front and rear

Delete factory installed black platform running boards

Color-coordinated Carpet with Carpeted Matching

Delete Trailer Tow Package, manual-folding, manually telescoping power glass trailer tow mirrors with heat, and 11,200 towing capacity. (Standard tow package will remain with 7,000 lbs. tow limit.)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101702 – POLICE VEHICLES*  **MODEL YEAR 2021 OR NEWER: FORD EXPEDITION SPECIAL SERVICES VEHICLE** |
| **Mandatory Specifications** |
| **FOUR WHEEL DRIVE** |
| **ENGINE:**  3.5 EcoBoost V6 |
| **FRONT SEATS:**  Heavy duty bucket seats |
| Covered with heavy duty cloth fabric |
| No center console |
| 6-way power adjusting driver seat required |
| **SECOND ROW SEATING:**  Heavy duty cloth fabric second row bench seat |
| **THIRD ROW SEATING:**  None; Storage Bins |
| **FLOOR COVERING:**  Vinyl floor covering |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Ford Expedition Special Services Vehicle** |

Possible options to be requested by agency:

Extended Length (MAX) Option

Second row 40/20/40 vinyl seating

Third row 60/40 cloth seating

Factory installed running boards

Heavy-duty trailer tow package (Includes 18” machined-faced aluminum wheels with painted pockets and 275/65R18 all terrain OWL tires in lieu of standard 17” steel wheels and tires **(standard length vehicle only, extended length (Max option) vehicle retains standard 17” steel wheels and tires),** Heavy-duty radiator, Integrated trailer brake controller, two (2) speed auto 4WD with neutral towing capability)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code*: 25101505 – Minivans or vans*  **MODEL YEAR 2021 OR NEWER: FORD TRANSIT VAN 250 AWD** |
| **Mandatory Specifications** |
| **ENGINE:**  3.5 liter V6 EcoBoost |
| **ALL WHEEL DRIVE** |
| **WHEEL BASE:**  147.6” |
| **ROOF HEIGHT:**  Medium – 100.8” |
| **CRUISE CONTROL:**  Factory installed required, including Adjustable Speed Limiting Device |
| **AIR CONDITIONING & HEATING:**  Factory installed front and rear heat and air conditioning |
| **ELECTRIC REAR WINDOW DEFROSTER:**  Manufacturer’s standard required |
| **REMOTE KEYLESS ENTRY SYSTEM:**  Remoted keyless entry system with minimum of four (4) keyless entry key FOBS |
| **OUTSIDE REAR VIEW MIRRORS:**  Long arm, power adjusting with turn signals |
| Heated required |
| **FRONT SEATS:**  10-way power adjusting driver and passenger seat required |
| Dark Gray cloth fabric |
| **BLUETOOTH:**  Factory Installed Bluetooth hands-free, includes dual USB ports and 4” multifunction display |
| **SAFETY:**  Pre-collision and post-collision auto braking |
| Lane alert |
| **SIDE DOOR:**  Manual sliding passenger side door with fixed privacy glass |
| **REAR DOORS:**  Dual rear doors with fixed privacy glass |
| **FOG LAMPS:**  Front fog lamps required |
| **FUEL TANK:**  Extended range 31-gallon fuel tank |
| **EXTERIOR UPGRADE OPTION:**  Chrome timed headlamps, three (3) bar grille with chrome surround, and full silver wheel covers |
| **AUXILIARY FUSE PANEL OPTION:**  Aux. fuse panel with interface connector, dual AGM batteries, and modified wiring system |
| **110 VOLT OUTLET:**  110 V / 400W outlet required |
| **REAR POWER POINT:**  12 volt power point located in rear of vehicle |
| **FLOOR COVERING:**  Vinyl floor covering front |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **WHEEL WELL LINER:**  Black, Front |
| **PAYLOAD:**  9070 GVWR |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Ford Transit 250** |

Possible options to be requested by agency:

Two (2) additional key with FOBS

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

|  |
| --- |
| UNSPSC Code: *25101505 – Minivans or vans*  **MODEL YEAR 2021 OR NEWER: FORD TRANSIT VAN 350 DUAL REAR WHEEL AWD** |
| **Mandatory Specifications** |
| **ENGINE:**  3.5 liter V6 EcoBoost |
| **ALL WHEEL DRIVE** |
| **WHEEL BASE:**  147.6” |
| **ROOF HEIGHT:**  High – 110.1” |
| **CRUISE CONTROL:**  Factory installed required, including Adjustable Speed Limiting Device |
| **AIR CONDITIONING & HEATING:**  Factory installed front and rear heat and air conditioning |
| **ELECTRIC REAR WINDOW DEFROSTER:**  Manufacturer’s standard required |
| **REMOTE KEYLESS ENTRY SYSTEM:**  Remoted keyless entry system with minimum of four (4) keyless entry key FOBS |
| **OUTSIDE REAR VIEW MIRRORS:**  Long arm, power adjusting with turn signals |
| Heated required |
| **FRONT SEATS:**  10-way power adjusting driver and passenger seat required |
| Dark Gray cloth fabric |
| **SIDE DOOR:**  Manual sliding passenger side door with fixed privacy glass |
| **REAR DOORS:**  Dual rear doors with fixed privacy glass |
| **FOG LAMPS:**  Front fog lamps required |
| **FUEL TANK:**  Extended range 31-gallon fuel tank |
| **EXTERIOR UPGRADE OPTION:**  Chrome timed headlamps, three (3) bar grille with chrome surround, and full silver wheel covers |
| **AUXILIARY FUSE PANEL OPTION:**  Aux. fuse panel with interface connector, dual AGM batteries, and modified wiring system |
| **110 VOLT OUTLET:**  110 V / 400W outlet required |
| **REAR POWER POINT:**  12 volt power point located in rear of vehicle |
| **FLOOR COVERING:**  Vinyl floor covering front |
| **FRONT LICENSE BRACKET:**  Manufacturer’s standard required |
| **WHEEL WELL LINER:**  Black, Front |
| **PAYLOAD:**  9,950 GVWR |
| **COLORS:**  Standard production solid color exterior and standard interior trim |
| Colors will be selected after award |
| **MANDATORY MODEL: Ford Transit 350** |

Possible options to be requested by agency:

Two (2) additional key with FOBS

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

C/S Code*: 25101702 POLICE VEHICLES*  1 TOTL TBD

**MISCELLANEOUS OPTIONS / FEATURES**

Line item shall be used for the purchase of miscellaneous vehicle options/features not specified herein. Prior to issuing a purchase order, the state agency shall contact the contractor to obtain the price for the option required.