Copyright September 2012, Division of Facilities Management, Design and Construction (FMDC)

SECTION 013513.31 – SITE SECURITY AND HEALTH REQUIREMENTS (DNR)

This section shall be used for all Missouri Departments of Agriculture, Economic Development, Natural Resources, Public Safety, Transportation, and Social Services projects (excluding Youth Services). Omit this section if any work will occur at the Departments of Corrections, Mental Health, State Schools, Youth Services, or OA Facilities.

1. GENERAL
   * + 1. RELATED DOCUMENTS
          1. Drawings and general provisions of the Contract including General and Supplementary Conditions, Bid Form, and other Division 1 Specification Sections apply to this Section.
       2. SUBMITTALS
          1. List of required submittals:

Materials Safety Data Sheets for all hazardous materials to be brought onsite.

Schedule of proposed shutdowns, if applicable.

A list of the names of all employees who will submit fingerprints for a background check, and the signed privacy documents identified below for each employee.

1. PRODUCTS (Not Applicable)
2. EXECUTION
   * + 1. ACCESS TO THE SITE
          1. The Contractor shall arrange with Facility Representatives to establish procedures for the controlled entry of workers and materials into the work areas at the Facility.
          2. The Contractor shall establish regular working hours with Facility Representatives. The Contractor must report changes in working hours or overtime to Facility Representatives and obtain approval twenty-four (24) hours ahead of time. The Contractor shall report emergency overtime to Facility Representatives as soon as it is evident that overtime is needed. The Contractor must obtain approval from Facility Representatives for all work performed after dark.
          3. The Contractor shall provide the name and phone number of the Contractor’s employee or agent who is in charge onsite; this individual must be able to be contacted in case of emergency. The Contractor must be able to furnish names and address of all employees upon request.

Determine acceptable working hours for construction activities with the Facility and revise paragraph below as appropriate.

* + - * 1. All construction personnel shall visibly display issued identification cards.

Omit paragraph below if not required by Facility.

* + - 1. FIRE PROTECTION, SAFETY, AND HEALTH CONTROLS
         1. The Contractor shall take all necessary precautions to guard against and eliminate possible fire hazards.

Onsite burning is prohibited.

The Contractor shall store all flammable or hazardous materials in proper containers located outside the buildings or offsite, if possible.

The Contractor shall provide and maintain, in good order, during construction fire extinguishers as required by the National Fire Protection Association. In areas of flammable liquids, asphalt, or electrical hazards, 15-pound carbon dioxide or 20-pound dry chemical extinguishers shall be provided.

* + - * 1. The Contractor shall not obstruct streets or walks without permission from the Owner’s Construction Representative and Facility Representatives.
        2. The Contractor’s personnel shall not exceed the speed limit of 15 mph while at the Facility unless otherwise posted.
        3. The Contractor shall take all necessary, reasonable measures to reduce air and water pollution by any material or equipment used during construction. The Contractor shall keep volatile wastes in covered containers, and shall not dispose of volatile wastes or oils in storm or sanitary drains.
        4. The Contractor shall keep the project site neat, orderly, and in a safe condition at all times. The Contractor shall immediately remove all hazardous waste, and shall not allow rubbish to accumulate. The Contractor shall provide onsite containers for collection of rubbish and shall dispose of it at frequent intervals during the progress of the Work.
        5. Fire exits, alarm systems, and sprinkler systems shall remain fully operational at all times, unless written approval is received from the Owner’s Construction Representative and the appropriate Facility Representative at least twenty-four (24) hours in advance. The Contractor shall submit a written time schedule for any proposed shutdowns.
        6. For all hazardous materials brought onsite, Material Safety Data Sheets shall be on site and readily available upon request at least a day before delivery.
        7. Alcoholic beverages or illegal substances shall not be brought upon the Facility premises. The Contractor’s workers shall not be under the influence of any intoxicating substances while on the Facility premises.
      1. DISRUPTION OF UTILITIES
         1. The Contractor shall give a minimum of seventy-two (72) hours written notice to the Construction Representative and the Facility Representative before disconnecting electric, gas, water, fire protection, or sewer service to any building.
         2. The Contractor shall give a minimum of seventy-two (72) hours written notice to the Construction Representative and Facility Representative before closing any access drives, and shall make temporary access available, if possible. The Contractor shall not obstruct streets, walks, or parking.

**END OF SECTION 013513.31**